Q & A

### Q: The depth or load counters are suddenly frozen on the PC?

### A: Restart the computer. It may take up to 2-3 restarts.

### Q: How do I connect the depth counter to the logger?

### A: Open the surface unit (silver box) and connect the depth-counter USB cable (otherwise connected to the raspberry PI) to a USB extension cable for use with the “logger laptop”.

### Q: How do I recalibrate the load and depth counters?

### A: The relevant parts of the manual are pasted on the walls of the drill cabin, else contact Aslak G. or Nicholas R.

### Q: Where are screenshots and log files saved?

### A: In the /mnt/logs directory (requires a USB pen be inserted into the surface unit front panel).

### 